Separation

Vertical separation 1000ft between identified aircraft – 5000ft between unidentified aircraft

Lateral separation at least 3nm between identified aircraft – 5nm between unidentified aircraft

Radar Vectoring

# Aircraft track

The path followed by the aircraft over the ground.

Have to adjust heading to allow for wind blowing aircraft off course